{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["询价表"],"read":"whole","date_system":"1900"}

{"sheet":"询价表","index":0,"n_rows":46,"n_cols":8,"rows_kept":46,"merged":[[0,0,0,7],[1,0,1,7],[12,2,12,5],[13,0,13,7],[24,2,24,5],[25,0,25,7],[37,2,37,5],[38,0,38,5],[40,0,40,7]]}
["汕头职业技术学院院本部互联网+明厨亮灶项目建设询价表"]
["一、第一食堂"]
["序号","选项","相关参数","单位","数量","综合单价","综合总价","备注"]
[1,"前端AI摄像机","DS-2CD2T2MCLZ/HJ；200万1/2.7”CMOS ICR红外阵列筒型网络摄像机；感兴趣区域：ROI支持三码流分别设置1个固定区域；智能报警：越界侦测,区域入侵侦测,场景变更侦测,人脸侦测,虚焦侦测，物品遗留侦测,物品拾取侦测,非法停车侦测,人员聚集侦测,徘徊侦测,快速移动侦测,进入区域侦测,离开区域侦测；红外照射距离最远可达：50米 ；支持智能后检索，配合NVR支持事件的二次检索分析；","台",4]
[2,"智能视频接入联网分析主机","iDS-6708NX/X-AI；配合EBG行业一体化平台(ISC)项目使用，配合云眸进行项目使用\n分析能力：图片分析8张/秒/GPU；支持实时视频分析，2路/GPU；支持视频轮巡分析，8路/GPU，轮巡间隔10~3600秒 可配\n支持定时抓图分析，8路/GPU，抓图间隔 3~3600秒 可配","套",1]
[3,"存储设备","4T专用硬盘","块",1]
[4,"交换机","DS-3E0109SP-E 8POE+1百兆 60W","套",1]
[5,"路由器","WAN口：2个10/100/1000Base-T以太网端口\nLAN口：3个10/100/1000Base-T以太网端口\n1个USB接口；1个Console口","套",1]
[6,"设备专用柜","壁式","台",1]
[7,"辅助材料","线材、管道、HDMI线、水晶头等配件","项",1]
["A","小计","-","-","-","-",{"$f":"SUM(G4:G10)","v":0}]
["B","施工调试费","-","-","-","-",{"$f":"G11*0.15","v":0}]
["C","总计","A+B",{"$nulls":3},{"$f":"G11+G12","v":0},"包含普通发票"]
["二、第二食堂"]
["序号","选项","相关参数","单位","数量","综合单价","综合总价","备注"]
[1,"前端AI摄像机","DS-2CD2T2MCLZ/HJ；200万1/2.7”CMOS ICR红外阵列筒型网络摄像机；感兴趣区域：ROI支持三码流分别设置1个固定区域；智能报警：越界侦测,区域入侵侦测,场景变更侦测,人脸侦测,虚焦侦测，物品遗留侦测,物品拾取侦测,非法停车侦测,人员聚集侦测,徘徊侦测,快速移动侦测,进入区域侦测,离开区域侦测；红外照射距离最远可达：50米 ；支持智能后检索，配合NVR支持事件的二次检索分析；","台",2,null,null,"新增炒菜区、洗菜区"]
[2,"智能视频接入联网分析主机","iDS-6708NX/X-AI；配合EBG行业一体化平台(ISC)项目使用，配合云眸进行项目使用\n分析能力：图片分析8张/秒/GPU；支持实时视频分析，2路/GPU；支持视频轮巡分析，8路/GPU，轮巡间隔10~3600秒 可配\n支持定时抓图分析，8路/GPU，抓图间隔 3~3600秒 可配","套",1]
[3,"存储设备","4T专用硬盘","块",1]
[4,"交换机","DS-3E0109SP-E 8POE+1百兆 60W","套",1]
[5,"路由器","WAN口：2个10/100/1000Base-T以太网端口\nLAN口：3个10/100/1000Base-T以太网端口\n1个USB接口；1个Console口","套",1]
[6,"设备专用柜","壁式","台",1]
[7,"辅助材料","线材、管道、HDMI线、水晶头等配件","项",1]
["A","小计","-","-","-","-",{"$f":"SUM(G16:G22)","v":0}]
["B","施工调试费","-","-","-","-",{"$f":"G23*0.15","v":0}]
["C","总计","A+B",{"$nulls":3},{"$f":"G23+G24","v":0},"包含普通发票"]
["三、职工食堂"]
["序号","选项","相关参数","单位","数量","综合单价","综合总价","备注"]
[1,"前端AI摄像机","DS-2CD2T2MCLZ/HJ；200万1/2.7”CMOS ICR红外阵列筒型网络摄像机；感兴趣区域：ROI支持三码流分别设置1个固定区域；智能报警：越界侦测,区域入侵侦测,场景变更侦测,人脸侦测,虚焦侦测，物品遗留侦测,物品拾取侦测,非法停车侦测,人员聚集侦测,徘徊侦测,快速移动侦测,进入区域侦测,离开区域侦测；红外照射距离最远可达：50米 ；支持智能后检索，配合NVR支持事件的二次检索分析；","台",7]
[2,"智能视频接入联网分析主机","iDS-6708NX/X-AI；配合EBG行业一体化平台(ISC)项目使用，配合云眸进行项目使用\n分析能力：图片分析8张/秒/GPU；支持实时视频分析，2路/GPU；支持视频轮巡分析，8路/GPU，轮巡间隔10~3600秒 可配\n支持定时抓图分析，8路/GPU，抓图间隔 3~3600秒 可配","套",1]
[3,"存储设备","4T专用硬盘","块",1]
[4,"交换机","DS-3E0109SP-E 8POE+1百兆 60W","套",1]
[5,"路由器","WAN口：2个10/100/1000Base-T以太网端口\nLAN口：3个10/100/1000Base-T以太网端口\n1个USB接口；1个Console口","套",1]
[6,"液晶电视","50寸","套",1,"-","-","甲方提供，无需报价"]
[7,"设备专用柜","壁式","台",1]
[8,"辅助材料","线材、管道、HDMI线、水晶头等配件","项",1]
["A","小计","-","-","-","-",{"$f":"SUM(G28:G35)","v":0}]
["B","施工调试费","-","-","-","-",{"$f":"G36*0.15","v":0}]
["C","总计","A+B",{"$nulls":3},{"$f":"G36+G37","v":0},"包含普通发票"]
["合计（三个食堂）",{"$nulls":5},{"$f":"G13+G25+G38","v":0},"包含普通发票"]
[1,"网络专线","保证每路摄像枪有独立2M上行带宽","条",3,0,{"$f":"E40*F40","v":0},"甲方提供，无需报价"]
["以上报价含税、运费、安装调试费，一年质保，实现接入濠江区明厨亮灶系统。"]
["供应商（公章）："]
[]
["联系人："]
[]
["联系电话："]